**Leslie Pool Close Out Checklist**

|  |  |  |
| --- | --- | --- |
| **DONE** | **CABLE RUN** | **DESCRIPTION OF TASK** |
|  | Run 1 (LP1) | Runs 1 and 2 – Extend two CAT5e cables from patch panel jacks 1 and 2 to Cash Wrap. Terminate with RJ45 jacks under the counter in the LEFT console. Label the jacks ‘LP1’ and ‘LP2’ to correspond with their respective patch panel jacks. |
|  | Run 2 (LP2) |
|  | Run 3 (LP3) | Extend two CAT5e cables from patch panel jacks 3 and 4 Cash Wrap. Terminate with RJ45 jacks under the counter in the CENTER console. Label the jacks ‘LP3’ and ‘LP4’ to correspond with their respective patch panel jacks. |
|  | Run 4 (LP4) |
|  | Run 5 (LP5) | Extend two CAT5e cables from patch panel jacks 5 and 6 to Cash Wrap. Terminate with RJ45 jacks under the counter in the RIGHT console. Label the jacks ‘LP5’ and ‘LP6’ to correspond with their respective patch panel jacks. |
|  | Run 6 (LP6) |
|  | Run 7 (LP7) | Extend two CAT5e cables from patch panel jacks 7 and 8 to the Water Test counter. Terminate with RJ45 jacks under the counter. Label the jacks ‘LP7’ and ‘LP8’ to correspond with their respective patch panel jacks. |
|  | Run 8 (LP8) |
|  | Run 9 (LP9) | (Wireless AP Network Connection) Extend one CAT5e cable from patch panel jack 9 to terminate at an RJ45 jack mounted on the ceiling near the back wall of the showroom, centered left to right. |
|  | Run 10 (LP10) | Extend one CAT5e cable from patch panel jack 10 to shop counter. Terminate with RJ45 jack under counter. Label the jack ‘LP10’ to correspond with the patch panel jack. |
|  | Run 11 (LP11) | Extend one CAT5e cable from patch panel jack 11 to Store Manager’s desk. Terminate with RJ45 jack. Label the jack ‘LP11’ to correspond with the patch panel jack |

|  |  |  |
| --- | --- | --- |
| **YES** | **NO** | **DESCRIPTION OF TASK** |
|  |  | Did you terminate the end of the cable for the Access Point with an RJ45? |
|  |  | Did you leave the AP cable exposed from the ceiling for the Installer to identify where the AP cable is located? |
|  |  | Did you install the surge Protector in the rack? |
|  |  | Have you completed testing? |
|  |  | Have you completed documentation of the testing? |
|  |  |  |
|  |  | **PHOTOS** |
|  |  | Have you taken the required photos? |
|  |  | Closeup and wide angle up of the rack |
|  |  | Close and wide angle up of the back board |
|  |  | Photo of AP Cable |
|  |  | Photo of each termination end point |
|  |  | Photos of the patch panel (labeled) |